<http://complextoreal.com/wp-content/uploads/2013/01/mft.pdf>

Matched filter – reduces additive noise

* There is a best filter as a function of transmitted shape
  + The “matched filter”
  + Maximize SNR, minimize probability of BER (bit error?)
* Receive s(t) + n(t)